# **GRÖNLID Corner sofa-bed, 4-seat, with open end/ Ljungen light red**

**Product details $1700**

Deep seat cushions with a top layer of fibre balls and plenty of comfortable back cushions make GRÖNLID sofa feel soft and inviting.The sofa's sections can be combined in different ways to get a size and shape that suits you. If you ever need a larger sofa, you can always add a section or two.

**Materials & care**

* **Frame, 2-seat sofa-bed section**
* **Back frame:**Solid wood, Plywood, Fibreboard, Particleboard, Polyurethane foam 20 kg/cu.m., Polyester wadding
* **Front rail:**Particleboard, Plywood, Polyurethane foam 20 kg/cu.m.
* **Metal parts:**Steel
* **Lining/ Lining:**Non-woven polypropylene
* **Seat cushion:**Polyester wadding, Polyester fibre balls, Highly resilient polyurethane foam (cold foam) 35 kg/cu.m., Non-woven polypropylene
* **Back cushion:**30% cut polyurethane foam/ 70% polyester fibres
* **Corner section frame**
* **Frame:**Solid wood, Fibreboard, Plywood, Polyurethane foam 20 kg/cu.m., Polyester wadding, Particleboard
* **Metal parts:**Steel
* **Leg:**Polypropylene plastic
* **Back fabric:**100 % polyester (100% recycled)
* **Frame 1-seat section**
* **Frame:**Solid wood, Plywood, Fibreboard, Polyester wadding, Polyurethane foam 20 kg/cu.m., Non-woven polypropylene, Particleboard
* **Metal parts:**Steel
* **Fitting:**Polypropylene plastic
* **Back fabric:**100 % polyester (100% recycled)
* **Frame footstool with storage**
* **Frame:**Plywood, Fibreboard, Polyurethane foam 20 kg/cu.m., Particleboard, Laminate (melamine)
* **Seat cushion:**Highly resilient polyurethane foam (cold foam) 35 kg/cu.m., Polyester wadding, Polyester fibre balls
* **Metal parts:**Steel, Epoxy/polyester powder coating
* **Leg:**Polypropylene plastic
* **Frame armrest**
* **Frame:**Solid wood, Plywood, Fibreboard, Polyurethane foam 30 kg/cu.m., Polyester wadding, Particleboard, Polyurethane foam 20 kg/cu.m.
* **Metal parts:**Steel
* **Leg:**Polypropylene plastic
* **Sofa-bed mechanism**
* **Layer glued slats:**Moulded layer-glued wood veneer, Adhesive resin as coating
* **Seat frame/ Seat frame:**Steel, Epoxy/polyester powder coating
* **Inner seat cushion corner section/ inner seat cushion**

Highly resilient polyurethane foam (cold foam) 35 kg/cu.m., Polyester wadding, Polyester fibre balls

* **Inner back cushion**

30% cut polyurethane foam/ 70% polyester fibres

* **Foam mattress**
* **Ticking:**64% polyester, 36% cotton
* **Comfort material:**Polyester wadding
* **Lining:**Non-woven polypropylene
* **Cover for 2-seat sofa-bed section**
* **Cover, other surfaces:**100% polyester
* **Back fabric/ Fabric:**100 % polyester (100% recycled)
* **Cover for corner section/ cover for footstool with storage/ cover for armrest**

100 % polyester (100% recycled)

* **Cover for 1-seat section**
* **Cover, other surfaces:**100% polyester
* **Fabric/ Back fabric:**100 % polyester (100% recycled)
* **Mattress coverFoam mattress**Machine wash, max 60°C, normal process.Do not bleach.Do not tumble dry.Do not iron.Do not dryclean.
* **Removable coverCover for 2-seat sofa-bed section/cover for corner section/cover for 1-seat section/cover for footstool with storage/cover for armrest**Machine wash, max 40°C, normal process.To be washed separately.Do not bleach.Do not tumble dry.Iron, max 110°C.Professional dry cleaning in tetrachloroethene and hydrocarbons, normal process.
* **FrameCorner sofa-bed, 4-seat**Wipe clean with a dry cloth.

## Product size

**Height including back cushions:**

104 cm (41 ")

**Height backrest:**

68 cm (26 3/4 ")

**Depth:**

98 cm (38 5/8 ")

**Width right:**

235 cm (92 1/2 ")

**Width left:**

271 cm (106 3/4 ")

**Seat depth:**

60 cm (23 5/8 ")

**Seat height:**

49 cm (19 1/4 ")

**Bed width:**

140 cm (55 1/8 ")

**Bed length:**

200 cm (78 3/4 ")

**Mattress thickness:**

12 cm (4 3/4 ")